From 338c6d7980947579d7419feeaa48ca8f9ae84086 Mon Sep 17 00:00:00 2001
From: sara <sara.halter@gmx.ch>
Date: Sat, 27 Nov 2021 16:02:16 +0100
Subject: Test FIR filter implemenatation / eigener FIR Block Gnur radio

---
 doc/thesis/chapters/implementation.tex | 7 ++++++-
 1 file changed, 6 insertions(+), 1 deletion(-)

(limited to 'doc/thesis/chapters/implementation.tex')

diff --git a/doc/thesis/chapters/implementation.tex b/doc/thesis/chapters/implementation.tex
index 27a8d41..91a1856 100644
--- a/doc/thesis/chapters/implementation.tex
+++ b/doc/thesis/chapters/implementation.tex
@@ -72,10 +72,15 @@ Here its possible to add some AWGN noise in the channel line. Different paramete
 
 To get a basic line for further simulations a 16QAM has been made. The results of this simulation are shown in \figref{fig:simul16QAM} and \figref{fig:simul16QAM_1} as the red Signal. In \tabref{tab:modulation_settings} some importer Parameter settings for a different modulation scheme are mentioned.
 
-A FIR-Filter was added in the Channel to create a time delay between tow paths. In \figref{fig:simul16QAM} the result includes a direct path and a delayed one. In the plot of \figref{fig:simul16QAM_1} the transmission line dosn't include a direct path. It's impotent to mention that the delay should be smaller than the symbol rate or a multiple of it. 
+A FIR-Filter was added in the Channel to create a time delay between tow paths. In \figref{fig:simul16QAM} the result includes a direct path and a delayed one. In the plot of \figref{fig:simul16QAM_1} the transmission line dosn't include a direct path. %It's impotent to mention that the delay should be smaller than the symbol rate or a multiple of it. (Stimmt dies , not sure any more)
 
 For the a first simulation with some fading the 16QAM simulation model has been extended with a FIR-Filter in the Chanel. The results of this simulation are shown in \figref{fig:simul16QAM} and \figref{fig:simul16QAM_1} as the blue Signal.
 
+%TO DO: übersetzen 
+Für das veranschaulichen des Fading effekts wurde ein eigener Block kreaiert und in den Channel implementiert. Dieser Block basiert auf einem FIR Filter. Es kann mit direcktem Pfad oder ohne dargestellt werden ( Line of Side ). Mit Hilfe des FIR filters wird die Verspätung der nebenpfaden dargestellt. Es ist möglich beliebig viele dieser Pfade mit unterschiedlicher stärke zu simulieren.
+
+
+
 
 \section{Hardware}
 
-- 
cgit v1.2.1

