From 921053182aaed15476738327112124db07ef432e Mon Sep 17 00:00:00 2001
From: Nao Pross <np@0hm.ch>
Date: Fri, 30 Jul 2021 19:39:00 +0200
Subject: HSR colors

---
 tex/model-hardware.tex | 18 +++++++++---------
 1 file changed, 9 insertions(+), 9 deletions(-)

(limited to 'tex/model-hardware.tex')

diff --git a/tex/model-hardware.tex b/tex/model-hardware.tex
index df0a220..c0ccedc 100644
--- a/tex/model-hardware.tex
+++ b/tex/model-hardware.tex
@@ -35,7 +35,7 @@ the other axis while gravitating towards the origin (project goal).
           ] {\desc};
       }
 
-      \draw[red, thick] (O) to ++(30:6)
+      \draw[hsr-mauve, thick] (O) to ++(30:6)
         node[
           above = 3mm,
           align = center,
@@ -48,10 +48,10 @@ the other axis while gravitating towards the origin (project goal).
         4/{Subblocks},
         5/{Top blocks, I/O}
       } {
-        \draw[red] (30:\r)
+        \draw[hsr-mauve] (30:\r)
           node[
             circle, minimum size = 2mm,
-            fill = red,
+            fill = hsr-mauve,
             outer sep = 0,
             inner sep = 0
           ] {}
@@ -63,7 +63,7 @@ the other axis while gravitating towards the origin (project goal).
           ] {\desc};
       }
 
-      \draw[blue, thick] (O) to ++(150:6)
+      \draw[hsr-blue, thick] (O) to ++(150:6)
         node[
           above = 3mm,
           align = center,
@@ -76,10 +76,10 @@ the other axis while gravitating towards the origin (project goal).
         4/{Subtasks},
         5/{Algorithm}
       } {
-        \draw[blue] (150:\r)
+        \draw[hsr-blue] (150:\r)
           node[
             circle, minimum size = 2mm,
-            fill = blue,
+            fill = hsr-blue,
             outer sep = 0,
             inner sep = 0
           ] {}
@@ -91,7 +91,7 @@ the other axis while gravitating towards the origin (project goal).
           ] {\desc};
       }
 
-      \draw[green!60!black, thick] (O) to ++(270:6)
+      \draw[hsr-lakegreen, thick] (O) to ++(270:6)
         node[
           below = 3mm,
           align = center,
@@ -104,10 +104,10 @@ the other axis while gravitating towards the origin (project goal).
         4/{Floorplan partitioning},
         5/{Chip or board}
       } {
-        \draw[green!60!black] (270:\r)
+        \draw[hsr-lakegreen] (270:\r)
           node[
             circle, minimum size = 2mm,
-            fill = green!60!black,
+            fill = hsr-lakegreen,
             outer sep = 0,
             inner sep = 0
           ] {}
-- 
cgit v1.2.1

