From 91a346c87debb3b5d949e2e138faf9d83c83b555 Mon Sep 17 00:00:00 2001
From: Nao Pross <np@0hm.ch>
Date: Mon, 20 Dec 2021 17:53:27 +0100
Subject: Add figure for measurements with hardware

---
 doc/thesis/chapters/implementation.tex | 12 ++++++++++--
 1 file changed, 10 insertions(+), 2 deletions(-)

(limited to 'doc/thesis/chapters/implementation.tex')

diff --git a/doc/thesis/chapters/implementation.tex b/doc/thesis/chapters/implementation.tex
index 4518611..9155b2e 100644
--- a/doc/thesis/chapters/implementation.tex
+++ b/doc/thesis/chapters/implementation.tex
@@ -1,6 +1,6 @@
 % vim: set ts=2 sw=2 noet spell:
 
-\chapter{Implementation}
+\chapter{Implementation} \label{chp:implementation}
 
 \section{Overview}
 
@@ -393,7 +393,7 @@ The numbers of tags used in this case are similar to the number of given values.
 		\SI{5.0}{\micro\second} & \(\SI{-7.0}{\decibel} \approx 0.1995\) \\
 		\bottomrule
 	\end{tabular}
-	\caption{Extended Typical Urban model (ETU) ETSI Standard PDP values for multipath fading propagation conditions. \cite{ETSI}. \label{tab:etsi-tap-values}}
+	\caption{Extended Typical Urban model (ETU) ETSI Standard PDP values for multipath fading propagation conditions \cite{ETSI}. \label{tab:etsi-tap-values}}
 \end{table}
 
 % \begin{figure}
@@ -515,4 +515,12 @@ Without those only the amplitudes could be seen in the Plots, with all the noise
 		Simulations with a dynamic fading channel model using PDP values of the Extended Typical Urban model (ETU) of the ETSI standard normative Annex B.2 in \cite{ETSI}. The color gradient represents progression in time.
 	}
 \end{figure}
+\newpage
+\begin{figure}
+	\centering
+	\input{figures/tikz/qpsk-hardware}
+	\caption{
+		TODO QPSK hardware
+	}
+\end{figure}
 \restoregeometry
-- 
cgit v1.2.1


From 90b4872276ad0e870fa5a43fd89c0028b61befe6 Mon Sep 17 00:00:00 2001
From: Nao Pross <np@0hm.ch>
Date: Mon, 20 Dec 2021 18:53:07 +0100
Subject: Minor corrections

---
 doc/thesis/chapters/implementation.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'doc/thesis/chapters/implementation.tex')

diff --git a/doc/thesis/chapters/implementation.tex b/doc/thesis/chapters/implementation.tex
index 9155b2e..7be0a1c 100644
--- a/doc/thesis/chapters/implementation.tex
+++ b/doc/thesis/chapters/implementation.tex
@@ -47,7 +47,7 @@ class myblock(gr.sync_block):
 
 \subsection{Dear PyGUI}\label{sec:GUI}
 
-To construct a graphical interface for a demonstration platform the Dear IMGUI (immediate graphical user interface) library was chosen, mainly for its ease of use, wide range of techincal capabilites and high refresh rate. Dear PyGUI (DPG) are the Python bindings for the Dear IMGUI library.
+To construct a graphical interface for a demonstration platform the Dear IMGUI (immediate mode graphical user interface) library was chosen, mainly for its ease of use, wide range of techincal capabilites and high refresh rate. Dear PyGUI (DPG) are the Python bindings for the Dear IMGUI library.
 
 The DPG GUI communicates with the GR flow graphs using the IP/UDP protocol. This decision to separate the project into two parts that communicate over the IP network was made because it is not very easy to extend the graphical interface of GRC without interfering with the sophisticated multi-threaded architecture of GR. Furthermore, this allows to have multiple correctly configure flow graph on disk and to choose which one to run and display on the graphical interface, instead of having a single flow graph whose parameters need to be changed each time.
 
-- 
cgit v1.2.1

